**LIST OF FIGURES**

[Figure 3.1 Canny Edge detection hysteresis threshold curve 8](#_Toc9772618)

[Figure 3.2 Edge detection example 8](#_Toc9772619)

[Figure 3.3 Example of Gaussian Blur 9](#_Toc9772620)

[Figure 3.4 Houghline geometry for straight line 10](#_Toc9772621)

[Figure 3.5 Houghline detection example 11](#_Toc9772622)

[Figure 3.6 TensorFlow object detection example 12](#_Toc9772623)

[Figure 3.7 AlexNet neural network layers 13](#_Toc9772624)

[Figure 3.8 Arduino Uno R3 layout 14](#_Toc9772625)

[Figure 3.9 NRF24L01 module 15](#_Toc9772626)

[Figure 3.10 NRF24L01 channels and spacing 16](#_Toc9772627)

[Figure 3.11 NRF24L01 pin breakout 16](#_Toc9772628)

[Figure 3.12 A 12 V DC geared motor 17](#_Toc9772629)

[Figure 3.13 Motor construction 18](#_Toc9772630)

[Figure 3.14 Fleming’s left-hand rule 18](#_Toc9772631)

[Figure 3.15 8 Channel relay module 19](#_Toc9772632)

[Figure 3.16 Relay circuitry connected to arduino 20](#_Toc9772633)

[Figure 4.1 Flow Chart for Lane Detection Algorithm 21](#_Toc9772634)

[Figure 4.2 Send Drive Command to Arduino via Serial Interface 22](#_Toc9772635)

[Figure 4.3 Object detection using Tensorflow on GPU 23](#_Toc9772636)

[Figure 4.4 Create training data 24](#_Toc9772637)

[Figure 4.5 Training Dataset using TensorFlow AlexNet on GPU 25](#_Toc9772638)

[Figure 4.6 Screenshot of the model training 25](#_Toc9772639)

[Figure 4.7 Using Trained model to drive the car 26](#_Toc9772640)

[Figure 4.8 Block Diagram of the project 27](#_Toc9772641)